**16121138-16121146 : T7104-12CNG50 LOCATION DIAGRAM**

 ****

10

12

13

5

4

Figure : Front



9

11

6

Figure : Front Right



8

8

5

7

3

1

2

Figure : Back

COMPONENTS

|  |  |  |
| --- | --- | --- |
| ITEM | QTY | DESCRIPTION |
| 1 | 1 | Filter, Parker J6NH-10CWC23-130B |
| 2 | 1 | Filter, Parker J6NX-4C2C23-130B |
| 3 | 1 | Ball Valve, Oasis BV706 / Actuator, Bi-Torq |
| 4 | 1 | Relief Valve, Mercer Series 91 |
| 5 | 1 | Meter, Micro-Motion CNG50 |
| 6 | 1 | Ball Valve, Oasis BV706 |
| 7 | 3 | Gauge, TGT 5000PSI  |
| 8 | 2 | Needle Valve, NoShok |
| 9 | 1 | Bleed Valve, |
| 10 | 1 | Pressure Transducer, |
| 11 | 1 | Pressure Switch, |
| 12 | 1 | Three-Way Valve,  |
| 13 | 1 | Explosion Proof Box, TGT |