**17011150: T7204-12CNG50 LOCATION DIAGRAM**

****

10(x2)


4

3

4

11

Figure : Front



9

7

8

12

Figure : Front Right (Typ Back Right)



7

5

4 (x2)

2 (x2)

1 (x2)

3

Figure : Back

COMPONENTS

|  |  |  |
| --- | --- | --- |
| ITEM | QTY | DESCRIPTION |
| 1 | 2 | Filter, Parker |
| 2 | 2 | Ball Valve, Oasis |
| 3 | 2 | Relief Valve, Mercer Series 91 |
| 4 | 2 | Meter, Micro-Motion CNG50 |
| 5 | 3 | Gauge, TGT 5000PSI |
| 6 | 3 | Needle Valve, NoShok |
| 7 | 3 | Bleed Valve |
| 8 | 2 | Pressure Transducer |
| 9 | 2 | Pressure Switch |
| 10 | 2 | Asco Redhat Solenoid Valve, |
| 11 | 1 | Explosion Proof Box, TGT |
| 12 | 2 | Ball Valve, Parker |